**Q40 Fencing & Gates Specification**

*To be read in conjunction with Preliminaries/General conditions*

Description: On ground/temporary perimeter security gate system

Standard: BS1722-14: 2017

Manufacturer: CLD Fencing Systems [info@cld-systems.com](mailto:info@cld-fencing.com)

Tel. 01270 764751 [www.cld-systems.com](http://www.cld-fencing.com)

**Product Reference:** **CLD FenceSafe SlideMaster Cantilever Manual Sliding Gate**

Description: Open mesh aluminium security gate system with steel mesh infill, installed on ground using CLD FenceSafe Base

Configuration: Single leaf sliding to left or right or double leaf

Infill Panels: Options to be chosen from the CLD range of mesh fencing panels to match fenceline. See mesh type Q40 for more information.

Heights: Various heights available to suit customer requirements. Please contact CLD for more information.

Nominal heights: n/a

Widths (Select as

required): Single leaf opening size from 2000mm to 6000mm

Double leaf opening size from 4000mm to 12000mm

Gate Construction: Gate consists of main aluminium upright tower. Main gate frame supported on custom made cantilever beam. Frame constructed from 75x75mm Aluminium box with mesh infill as above.

Fixing: Main tower, park post and support rollers to be fixed to a temporary moveable base.

Locking: Manual locking options available

Finish: Polyester powder-coated to match mesh infill panels.

Any RAL colour

Foundations: Installed using a steel base with concrete ballast to suit gate width.

Warranty: Minimum of 15 years against manufacturing defects.

Notes: All dimensions are nominal, for further information please contact CLD Fencing Systems.

Information is correct at time of production. As part of our policy of continuous improvement, we reserve the right to alter product specification without notice.