**Q40 Fencing & Gates Specification**

*To be read in conjunction with Preliminaries/General conditions*

Description: Perimeter security fencing panel system

Standard: BS1722-14: 2017

Manufacturer: CLD Physical Security Systems Info@cld-systems.com

Tel. 01270 764751 [www.cld-systems.com](http://www.cld-fencing.com)

**Product Reference:** **CLD SportsRail Spectator Rail and Velodrome Fencing**

Panel width: Dependent on infill choice

Wire diameter: Wire diameter dependant on infill choice. Tube diameter - 48.6mm or 60.3mm

Mesh size: Dependent on infill choice

Available heights

Select as required: 900mm to 1390mm

Nominal heights: 0.9m to 1.39m

Finish: Polyester powder-coated to 60-80 microns or 160-200 microns with marine grade and metallics. Any RAL colour available

Top edge projection: n/a

Panel installation: Bottom of panel minimum 40mm above final ground level

Topping options: n/a

Posts: SHS or CHS dependant on application with CHS top rail, galvanised after manufacture and polyester powder-coated to match fencing

Maximum post

Centres: 2520mm

Warranty: Minimum of 15 years against manufacturing defects.

Notes: All dimensions are nominal, for further information please contact CLD Fencing Systems.

Information is correct at time of production. As part of our policy of continuous improvement, we reserve the right to alter product specification without notice.