**Q40 Fencing & Gates Specification**

*To be read in conjunction with Preliminaries/General conditions*

Description: Netting to integrate with Sports Fencing Systems

Manufacturer: CLD Fencing Systems

Tel. 01270 764751 [www.cld-fencing.com](http://www.cld-fencing.com)

**Product Reference: CLD Ball Stop Sports Netting**

Integration: Ball Stop polypropylene netting. Easily integrates with any fencing system, particularly Dulok Sports

Netting Width: To suit fence system

Net diameter: Variable

Mesh size: To suit customer requirements:
25 x 25mm, 50 x 50mm, 100 x 100mm as standard (other options available)

Height: 500mm to 10000mm

Nominal height: 0.5 to 10m

Finish: Polyester powder-coated to minimum 80 microns.

Any RAL colour

Netting installation: Fits to posts easily, with strong line wire added for support

Posts: SHS, galvanised after manufacture and polyester powder-coated to match fencing

Post dimensions: To suit fence system

Maximum post

Centres: To suit fence system

Fixings: To suit fence system

Warranty: Minimum of 12 months against manufacturing defects

Notes: All dimensions are nominal, for further information please contact CLD Fencing Systems.

Information is correct at time of production. As part of our policy of continuous improvement, we reserve the right to alter product specification without notice.